|  |
| --- |
| What symbols are used to indicate different types of brakes, as listed in Region B8? |
| What is the minimum required color depth and display size for the LCD module in the KAVACH Loco Pilot's Operation-cum-indication Panel (LP-OCIP (DMI))? |
| According to the document, how does the KAVACH system provide both visual and audible information to the loco pilot? |
| How does the KAVACH system communicate direction information to the loco pilot? |
| Which route image is displayed furthest from the vertical boundary line, and which is displayed closest? |
| How many routes and their corresponding images are to be displayed to the loco pilot? |
| What type of information is provided for direction, and how many different directions are indicated? |
| What color is the area between the current speed and the permissible speed when the system is applying the brakes to stop the train? |
| What key should be used to enter the Manual Brake Test mode and what is the corresponding screen name? |
| What is the size and resolution of the default display screen? |
| What should the user do after pressing a key from K1 to K7 to confirm the selection? |
| What text colour is used for all given text unless a specific colour is mentioned? |
| Could you please outline the introduction of this document? |
| What is the scope of this document? |
| Extract images and display |
| Responding for one word questions such as Goods, Keys and showing all instances with clause numbers |
| How to avoid misguiding information |